**Evaluation Criteria and Requirements Open Issues**

**Evaluation Criteria**

|  |  |
| --- | --- |
| **Potential Evaluation Criteria** | **Evaluation Criteria Recommended to Task Force** |
| EPoC Delay using EPoC Delay Model [1]  [1] Andrea Garavaglia, Ed Boyd, Rick Li, Bill Powell, Hesham ElBakoury, and David Barr, “EPoC Performance Model Delay and Efficiency,” September 2012 | EPoC Delay using EPoC Delay Model [1]  [1] Andrea Garavaglia, Ed Boyd, Rick Li, Bill Powell, Hesham ElBakoury, and David Barr, “EPoC Performance Model Delay and Efficiency,” September 2012 |

**Requirements**

|  |  |
| --- | --- |
| **Potential Requirement** | **Evaluation Criteria Recommended to Task Force** |
| The standard shall support a downstream data rate of at least 1.6 Gb/s at the MAC/PLS service interface, in a 192-MHz OFDM channel, in baseline channel conditions | The standard shall support a downstream data rate of at least 1.6 Gb/s at the MAC/PLS service interface, in a 192-MHz OFDM channel, in baseline channel conditions  (Adopted by the Task Force Nov 2012) |
| The MAC/PLS data rate shall scale linearly with the number of OFDM channels, in baseline channel conditions | The MAC/PLS data rate shall scale linearly with the number of OFDM channels, in baseline channel conditions  (Discussed by the Task Force Nov 2012, but not approved by the Task Force) |