

SYSTEM DESCRIPTION: Host Board-Connector-Module
HOST PCB DESCRIPTION: 154.4milS (3.9116mm) THICK, 16 LAYERS, Megtron7N, MICROVIA TO LAYER 15 ROUTE, 3.75mil Stub, 8.5" 5.3-6.45-5.3mil DIFFERENTIAL TRACES
CONNECTOR DESCRIPTION: TE OSFP SMT CONNECTOR
MODULE CONNECTOR:  39.4mils (1mm) THICK, 6 LAYERS, Megtron7N, TOP LAYER MICROVIA TO LAYER 02 ROUTE & BOT LAYER MICROVIA TO LAYER 5 ROUTE, 1.5" 6.3mil SE TRACES

DATA DESCRIPTION: MEASURED 4-port S-parameter 10MHZ TO 50GHZ
CALIBRATION: SOLT CALIBRATION, KEYSIGHT N4693-60003 ELECTRONIC CALIBRATION MODULE 10MHZ-50GHZ
TEST EQUIPMENT: KEYSIGHT PNA NETWORK ANALYZER N5225A

PORT 1 -----> PORT 2
PORT 3 -----> PORT 4