Contact Name:
	Howard Frazier

Contact Email:
	hfrazier@broadcom.com

What type of assignment/registration are you requesting?

Assignment of the following additions to the IANAifMauTypeListBits textual convention, immediately following b1000BasePX20U(53) -- 1000BASE-PX20U:

	b10GbaseT(xx) -- 10GBASE-T
	b10GbaseLRM(xx) -- 10GBASE-LRM
	b1000baseKX(xx) -- 1000BASE-KX
	b10GbaseKX4(xx) -- 10GBASE-KX4
	b10GbaseKR(xx) -- 10GBASE-KR
	b10G1GbasePRXD1(xx) -- 10/1GBASE-PRX-D1 
	b10G1GbasePRXD2(xx) -- 10/1GBASE-PRX-D2
	b10G1GbasePRXD3(xx) -- 10/1GBASE-PRX-D3
	b10G1GbasePRXU1(xx) -- 10/1GBASE-PRX-U1
	b10G1GbasePRXU2(xx) -- 10/1GBASE-PRX-U2
	b10G1GbasePRXU3(xx) -- 10/1GBASE-PRX-U3
	b10GbasePRD1(xx) -- 10GBASE-PR-D1
	b10GbasePRD2(xx) -- 10GBASE-PR-D2
	b10GbasePRD3(xx) -- 10GBASE-PR-D3
	b10GbasePRU1(xx) -- 10GBASE-PR-U1
	b10GbasePRU3(xx) -- 10GBASE-PR-U3

Assignment of the following additions to the IANAifMauAutoNegCapBits textual convention, immediately following b1000baseTFD(15) -- 1000BASE-T full duplex mode:

	b10GbaseT(xx) -- 10GBASE-T
	b1000baseKX(xx) -- 1000BASE-KX
	b10GbaseKX4(xx) -- 10GBASE-KX4
	b10GbaseKR(xx) -- 10GBASE-KR

Which registry are you requesting this assignment/registration be made in?

The assignment of the IANAifMauTypeListBits and IANAifMauAutoNegCapBits textual conventions is contained in the IANA-MAU-MIB, which is currently published as IETF RFC 4836. The IEEE 802.3 Ethernet Working Group is currently working on a project, known as IEEE P802.3.1, that will update and republish the IETF RFCs that are relevant to the management of Ethernet interfaces, including the contents of RFC 4836.

If possible, please give a brief description of why you need this assignment/registration:

The new MAU types and the associated AutoNeg capability bits listed above were specified in recently approved amendments to IEEE Std 802.3, including IEEE Std 802.3an-2006, IEEE Std 802.3aq-2007, IEEE Std 802.3ap-2007, and IEEE Std 802.3av-2009. The assignments will be reflected in Clause 14 of IEEE P802.3.1, “IEEE Draft Standard for Management Information Base (MIB) definitions for Ethernet.”

Additional Information. Please include a reference to the specification or RFC (if available) that defines this number or name space: 

IEEE Std 802.3-2008, subclauses 30.5.1.1.2 aMAUType and 30.6.1.1.5 aAutoNegLocalTechnologyAbility.